R1350 YA105 corrected LED map test.
Only change from the booted four-channel build: System yellow GPIO7 polarity restored to active-low based on hardware observation. Internet yellow stays on the original-kernel GPIO14.
GPIO5/7/8/14 are all active-low. No pinmux override, WAN daemon, or wireless-default changes.
