Device: Xiaomi Router 4 Pro R1350
Status: TEST / not yet boot-tested on physical device
OpenWrt branch: openwrt-24.10
OpenWrt commit: 924f06e76cd73e24d39691a4de621bdcae80a756
Kernel: Linux 6.6.144
Kernel build identity: nyarime@naixi.net
Target: ath79/generic
Profile: xiaomi_mi-router-4-pro-r1350
PCI 5GHz: 168c:0056 (QCA9888)
ART: flash 0x60000 size 0x10000 read-only
2.4G calibration: ART+0x1000 size 0x440
5G pre-calibration: ART+0x5000 size 0x2F20
Firmware partition: flash 0x200000 size 0xE00000
